## Master Cylinder Disassembly

1. | Remove the circlip (A) while pushing in the secondary piston (B).

2. | Remove the reservoir (A).

3. | Remove the stop pin (B) while pushing in the secondary piston (C).

4. | Remove the secondary piston (A) and primary piston (B).

5. | Remove the reservoir seal (A) from the reservoir cap (B).

6. | Remove the strainer(C) and grommets (D) from the reservoir (E). NOTE: When reservoir and master cylinder body are separated, replace the grommets with new ones.