## DTC Troubleshooting: 67

DTC: 67 | Torque Sensor I/F Circuit

1. | Clear the DTC.

2. | Start the engine.

3. | Turn the steering wheel from lock to lock several time, and wait 10 seconds or more. Does the EPS indicator come on? YES - Go to 4. NO - The system is OK at this time.n

4. | Stop the engine, and verify the DTC. Is DTC 67 indicated? YES - Check for loose EPS control unit connectors. If necessary, substitute a known-good EPS control unit and recheck.n NO - Perform the appropriate troubleshooting for the code indicated.n