## Door Lock Knob Switch Test - With Super Locking

## With Super Locking (Driver's door):

1. | Remove the driver's door panel.

2. | Disconnect the 6P connector (A) from the super locking actuator.

3. | Check for continuity between the terminals. There should be continuity between the No. 3 and No. 4 terminals when the door lock knob switch is LOCK position. There should be continuity between the No. 1 and No. 4 terminals when the door lock knob switch is UNLOCK position.

## With Super Locking (Passenger's door):

1. | Remove the passenger's door panel.

2. | Disconnect the 6P connector (A) from the super locking actuator.

3. | Check for continuity between the terminals. There should be continuity between the No. 1 and No. 4 terminals when the door lock knob switch is UNLOCK position.