## Windshield Wiper Motor Test

## Windshield:

1. | Remove the wiper arms, hood seals and cowl covers.

2. | Disconnect the 5P connector (A) from the wiper motor (B).

3. | Test the motor by connecting battery power to the No. 2 terminal and ground the No. 1 terminal of the wiper motor 5P connector. The motor should run. If the motor does not run or fails to run smoothly, replace the motor.

4. | Connect an analog voltmeter between the No. 5 (+) and No. 3 (-) terminals, and run the motor at low or high speed. The voltmeter should indicate 0 V and 4 V or less alternately.