## A/T Shift Lock Solenoid Replacement

1. | Remove the center console.

2. | Remove the A/T gear position indicator panel light socket (A) from the indicator panel (B), then remove the bulb (C) from the socket.

3. | Remove the shift lock solenoid/park pin switch connector (D) from the shift lever bracket base (E), then remove the connector.

4. | Remove the park pin switch connector (F).

5. | Release the lock tab (G) securing the shift lock solenoid, then remove the shift lock solenoid (H).

6. | Install the shift lock solenoid plunger (I) and spring (J) in the new shift lock solenoid.

7. | Install the shift lock solenoid by aligning the joint (K) of the shift lock solenoid plunger with the tip of the shift lock stop (L).

8. | Install the A/T gear position indicator panel light bulb in the panel light socket, then install the panel light socket in the A/T gear position indicator panel.

9. | Route the harness (L) through the shift lever bracket base, and connect the shift lock solenoid/park pin switch connector, then install it on the bracket base.

10. | Connect the park pin switch connector.

11. | Check that the shift lock releases when the shift lock release is pushed, and check that it locks when the shift lock release is released.

12. | Install the center console.