## M/T Mainshaft Disassembly

1. | Remove the ball bearing, tapered cone ring, distance collar, synchro ring and 5th synchro sleeve.

2. | Support 5th gear (A) on steel blocks, and press the mainshaft out of the 5th synchro hub (B). Use of a jaw-type puller can cause damage to the gear teeth.

3. | Support the 3rd gear (A) on steel blocks, and press the mainshaft out of the 3rd/4th synchro hub (B). Use of a jaw-type puller can cause damage to the gear teeth.