## Tailgate Lock Cylinder Replacement

NOTE: Put on gloves to protect your hands.

1. | Remove the tailgate lower trim panel.

2. | Disconnect the cylinder switch connector (A) (with cylinder switch) or the cylinder rod (B) (without cylinder switch), and detach it from the tailgate. With cylinder switch: Without cylinder switch:

3. | Remove the bolt securing the lock cylinder (A), then remove the lock cylinder by turning it.

4. | Install the lock cylinder in the reverse order of removal, and note these items: Make sure the connector is plugged in properly (for some models). Make sure the tailgate opens properly and locks securely.