## VSA OFF Switch Test

1. | Remove the VSA OFF Switch (A) from the switch panel.

2. | Disconnect the VSA OFF Switch 5P connector.

3. | Check for continuity between the VSA OFF Switch 5P connector terminal No. 1 and No. 2. There should be continuity when the switch is pushed.

4. | Check for continuity between the VSA OFF Switch connector terminal No. 4 and No. 5. There should be continuity at all times.