## Power Mirror Switch Test/Replacement

1. | Remove the driver's side dashboard side cover.

2. | Push the power mirror switch (A) out from the dashboard.

3. | Disconnect the 13P connector (B) from the switch.

4. | Check for continuity between the terminals in each switch position according to the table. Mirror Switch: Defogger Switch: Retract Switch:

5. | If the continuity is not as specified, replace the switch.