## DTC Troubleshooting: 13-1, 13-2

DTC 13-1, 13-2: | Internal Failure of the Driver's Side Impact Sensor

1. | Erase the DTC memory.

2. | Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off. Does the SRS indicator stay on? YES - Replace the driver's side impact sensor.n NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures.