## Inner Glove Box Removal/Installation

SRS components are located in this area. Review the SRS component locations, and the precautions and procedures in the SRS section before performing repairs or service.
NOTE:

- When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
- Take care not to scratch the dashboard and related parts.
- LHD is shown, RHD is symmetrical.

1. | Open the glove box lid.

2. | Gently pull out the inner glove box (A) to detach the clips, then remove it.

3. | Install the glove box in the reverse order of removal. Insert a rib (B) on back of the box to the holder (C) of the steering hanger beam.