## Rear Window Wiper Motor Test

## Rear Window

1. | Open the tailgate, and remove the tailgate lower panel.

2. | Disconnect the 4P connector (A) from the wiper motor (B).

3. | Test the motor by connecting battery power to the No. 1 terminal and ground the No. 3 terminal of the wiper motor. The motor should run. If the motor does not run or fails to run smoothly, replace the motor.

4. | Connect an analog voltmeter between the No. 4 (+) and No. 2 (-) terminals, and run the motor. The voltmeter should indicate 0 V and 4 V or more alternately. (With rear window intermittent wiper)