## Radiator and Fan Replacement

1. | Drain the engine coolant.

2. | Remove the front bumper, and front bumper beam.

3. | Remove the condenser upper mount brackets.

4. | Remove the upper bracket and cushions.

5. | Remove the upper radiator hose, lower radiator hose and automatic transmission fluid (ATF) cooler hose.

6. | Disconnect the fan motor connector, and remove the upper bracket and cushion, then pull up the radiator.

7. | Remove the fan shroud assemblies and other parts from the radiator.

8. | Install the radiator in the reverse order of removal. Make sure the upper and lower cushions are set securely.

9. | Install the condenser upper mount brackets.

10. | Install the front bumper beam, and apply body paint to the mounting bolts, then install the front bumper.

11. | Fill the radiator with engine coolant and bleed the air.