## DTC Troubleshooting: 62

DTC: 62 | EPS Control Unit Internal Circuit(Fail-safe Relay Stuck ON)

1. | Clear the DTC.

2. | Start the engine. Does the EPS indicator come on? YES - Go to 3. NO - The system is OK at this time.n

3. | Stop the engine, and verify the DTC. Is DTC 62 indicated? YES - Check for loose EPS control unit connectors.If necessary, substitute a known-good EPS control unit and recheck.n NO - Perform the appropriate troubleshooting for the code indicated.n