## Power Mirror Actuator Test

1. | Remove the door panel.

2. | Disconnect the 6P *1 (or 3P *2) connector (A) from the power mirror actuator

3. | Check actuator operation by connecting power and ground according to the table.

4. | If the mirror fails to work properly, replace the mirror actuator.

### Defogger Test:

5. | Check for continuity between the No. 1 and No. 2 terminals of the 6P connector. There should be continuity.

### Retract Switch:

6. | Check actuator operation by connecting battery power and ground according to the table.

7. | If the retract actuator fails to work properly, replace the mirror.