### Maintenance Schedule for Normal Conditions - European Model

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule do not apply.

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | l | l | l | l | l | l | l | l | l | l
Replace engine oil filter | l | l | l | l | l | l | l | l | l | l
Inspect front and rear brakes Check the brake pad and disc thickness. Check for damage and cracks Check the wheel cylinder for leaks Check the brake linings for cracking, glazing, wear and contamination Check the calipers for damage, leaks, and tightness | l | l | l | l | l | l | l | l | l | l
Check parking brake adjustment | l | l |  | l |  | l |  | l |  | l
Check lights alignment Check the position of the headlights | l | l | l | l | l | l | l | l | l | l
Test drive (noise, stability, dashboard operation) Check for road stability, noise, vibration and dashboard operation. | l | l | l | l | l | l | l | l | l | l
Visually inspect the following items: Check for correct installation and position, check for cracks, deterioration, rust, and leaks. Check tightness of screws, nuts, and joints. If necessary, retighten.
Tie-rod ends, steering gearbox, and boots Check rack grease and steering linkage. Check the boot for damage and leaking grease | l | l | l | l | l | l | l | l | l | l
Suspension components Check the bolts for tightness Check all dust cover for deterioration and damage
Driveshaft boots Check the boot and boot band for cracks Check rack grease
Brake hoses and lines (including ABS) Check the master cylinder, proportioning control valve and ABS modulator and leakage
All fluid levels and condition of fluid Check levels and check for leaks. If necessary, add engine coolant, MTF, ATF, brake fluid, windshield fluid, and battery fluid.
Exhaust system Check the exhaust pipe and muffler for damage, leaks and tightness

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Fuel lines and connections Check fuel lines for loose connections, cracks and deterioration. Retighten loose connections and replace any damaged parts | l | l | l | l | l | l | l | l | l | l
Tyre condition Check for pressure, puncture, cuts, and irregular thread wear.
Replace air cleaner element | Every 40,000 km (24,000 miles)
Replace spark plugs
Inspect valve clearance
Inspect and adjust drive belts Check for cracks, damage, deflection and tension |  | l |  | l |  | l |  | l |  | l
Replace dust and pollen filter | Every 30,000 km (18,000 miles) or 1 year
Replace fuel filter |  |  |  |  |  | l |  |  |  |
Inspect idle speed |  |  |  |  |  | l |  |  |  |
Replace manual transmission fluid Use genuine Honda Manual Transmission Fluid (MTF) | Every 120,000 km (72,000 miles) or 8 years
Replace CVT fluid Use genuine Honda ATF-Z1 | At 80,000 km (48,000 miles) or 5 years, then replace every 60,000 km (36,000 miles) or 4 years
Replace engine coolant Use genuine Honda All Season Antifrezee/Coolant Type 2 | At 200,000 km (120,000 miles) or 10 years, then replace every 100,000 km (60,000 miles) or 5 years
Replace brake fluid Use only DOT 3 or DOT 4 brake fluid (We recommend Genuine Honda Brake Fluid). Check that brake fluid level between the upper and lower marks on the reservoir | Every 3 years