## Wiper/Washer Switch Test/Replacement

1. | Remove the steering column covers.

2. | Disconnect the 14P connector (A) from the wiper/washer switch (B). LHD type and KE model: RHD type except KE:

3. | Remove the two screws, then pull out the wiper/washer switch.

4. | Inspect the connector terminals to be sure they are all making good contact. If the terminals are bent, loose or corroded, repair them as necessary, and recheck the system. If the terminals look OK, check for continuity between the terminals in each switch position according to the tables. If there is no continuity, replace the switch. Windshield : Rear window:
The wiper switch is combined with the windshield wiper intermittent control circuit, so that you cannot isolate the No. 9 terminal to check it. Instead, do the input test at this connector terminal on page 22-160. If the input test is OK, but the windshield wiper intermittent function has failure; the switch must be faulty.