## Side Sill Panel Replacement

1. | Remove the side sill panel.
-1 | Remove the front clip (A) and expansion clips (B).
-2 | Slide the side sill panel (C) forward, and remove it. The side clips (D) will stay in the body.
-3 | Remove the side clips from the body.

2. | Replace any damaged clips.

3. | Install the side clips on the side sill panel.

4. | Hold the panel up, and fit all the side clips into the holes in the body, then push on the panel until the clips snap into place.

5. | Install all the expansion clips and front clip.