## Resetting the Power Window Control Unit - With UP-AUTO Function

Resetting the power window control unit is required after performing the following procedures:

- Shutdown of the battery power
- Shutdown of the electric power caused by both No. 21 (10A) and No. 2 (20A) fuses in the under-dash fuse/relay box.
- Open circuit caused by disconnected 20P connector from the power window master switch
- Removal of the regulator, glass or glass run channel

1. | Make sure the glass is installed properly.

2. | Close the driver's door.

3. | Turn the ignition switch OFF.

4. | Remove the No. 2 (20A) fuse in the under-dash fuse/relay box

5. | Turn the ignition switch ON (II).

6. | After 1 second, turn the ignition switch OFF.

7. | After 5 seconds, install the No. 2 (20A) fuse to the under-dash fuse/relay box.

8. | Make sure the driver's window does not work in AUTO with the ignition switch ON (II).

9. | Turn the ignition switch START (III) and start the engine.

10. | Move the driver's window all the way down by manual DOWN of the driver's power window switch.

11. | Open the driver's door.

12. | Move the driver's window all the way up by manual UP of the driver's power window switch and hold on for 1 second.

13. | If the window does not work in AUTO, reset the power window master switch according to the above procedures again.