## DTC Troubleshooting: 52

DTC 52: | Motor Stuck OFF

1. | Check the No. 4 (30 A) fuse in the under-hood fuse/relay box. Is the fuse OK? YES - Reinstall the fuse, and go to 2. NO - Replace the fuse, and recheck. If fuse is blown, go to 4.

2. | Disconnect the VSA control unit 46P connector.

3. | Mesure the voltage between VSA control unit 46P connector terminal No. 45 and body ground. Is there battery voltage? YES - Go to 4. NO - Repair open in the wire between No. 4 (30 A) fuse in the under-hood fuse/relay box and VSA modulator-control unit.n

4. | Clear the DTCs using the HDS.

5. | Test-drive the vehicle at 15 km/h (9 mph) or more.

6. | Check the DTCs using the HDS. Does the ABS indicator come on, and are DTC 52 indicated? YES - Check for loose or poor connections in the VSA control unit 46P connector. If connections are good, replace the VSA modulator-control unit.n NO - The system is OK at this time.n