## A/C Condenser Replacement

1. | Recover the refrigerant with a recovery/recycling and charging station.

2. | Remove the front bumper.

3. | Remove the bolt and the nut, then disconnect the discharge line (A) and the receiver line (B) from the condenser. Plug or cap the lines immediately after disconnecting them to avoid moisture and dust contamination.

4. | Remove the mounting bolts and the upper brackets (A), then remove the condenser (B) by lifting it up. Be careful not to damage the condenser fins when removing the condenser.

5. | Install the condenser in the reverse order of removal, and note these items. If you're installing a new condenser, add refrigerant oil (KEIHIN SP-10). Replace the O-rings with new ones at each fitting, and apply a thin coat of refrigerant oil before installing them. Be sure to use the correct O-rings for HFC-134a (R-134a) to avoid leakage. Immediately after using the oil, reinstall the cap on the container, and seal it to avoid moisture absorption. Do not spill the refrigerant oil on the vehicle; it may damage the paint; if the refrigerant oil contacts the paint, wash it off immediately. Be careful not to damage the condenser fins when installing the condenser. Charge the system .