## Keyless Entry Transmitter Test

Special Toolds Required
Keyless Entry Checker ( 07MAJ-SP00400)

NOTE:

- If the doors unlock or lock with the transmitter, but the LED on the trnsmitter dose not come on, the LED is faulty; replace the transmitter.
- If any door is open, you cannot lock the doors with the transmitter.
- If you unlock the doors with the transmitter, but do not open any of the doors within 30 seconds, the doors relock automatically.
- The doors do not lock or unlock with the transmitter if the ignition key inserted in the ignition switch.

1. | Put on transmitter (A) behind the keyless entry checker (B).

2. | Press the door lock button. If the indicator light comes on, the transmitter is OK. If the indicator light dose not come on, check for: a dead or low battery. faulty transmitter.

### Battery Replacement

3. | Removed the screw abd transmitter cover.

4. | Replace the battery and recheck. If the indicator light dose not come on, replace the transmitter.

5. | After replacement, do the transmitter programming, and register the immobilizer system with the HDS.