## Door Lock Switch Test

1. | Remove the power window master switch.

2. | Disconnect the 3P connector from the power window master switch.

3. | Check for continuity between the terminals. There should be continuity between the No. 1 and No. 2 terminals when the door lock switch is in the LOCKED position. There should be continuity between the No. 2 and No. 3 terminals when the door lock switch is in the UNLOCKED position.