## Heater Control Panel Disassembly and Reassembly

NOTE: LHD type is shown, RHD type is symmetrical.

1. | Remove the heater fan switch (A), the air mix control cable (B), the mode control cable (C), and the recirculation control cable (D).

2. | Widen the cable stops (A) in the cable holder (B) using a snap ring pliers, then pull out the control cable (C).

3. | Hook the tip of the new control cable to the lever or slider, then push the cable housing into the cable holder until it locks into place.

4. | After assembly, check that the lever slides or the dial turns smoothly through the full stroke from right to left.