## Rear License Trim Replacement

NOTE: Put on gloves to protect your hands.

1. | Remove these items: Tailgate lower trim panel. Rear window wiper motor.

2. | From inside the tailgate, remove the bolts (A) securing the rear license trim (B).

3. | From inside the tailgate, release the clips (C, D) while holding the rear license trim.

4. | Remove the rear license trim (A). Take care not to scratch the tailgate.

5. | Install the trim in the reverse order of removal, and note these items: Replace any damaged clips. Do not roll up the lip (E) of the rear window rubber dam. If necessary for proper attachment, set a plastic plate between the lip and trim. Install the top edge of the trim while sliding a plastic plate sideward. Be careful not to cut the lip.