## Ignition Key Switch Test

NOTE: For more key-in beeper information, refer to the circuit diagram and input test.
When the ignition key is not removed, the key-in beeper in the gauge assembly senses ground through the closed ignition key switch. When you open the driver's door, the beeper circuit senses ground through the closed door switch.

1. | Remove the steering column upper and lower covers.

2. | Disconnect the 6P connector.

3. | Check for continuity between the No. 1 and No. 2 terminals. There should be continuity with the key in the ignition switch. There should be no continuity with the key removed.