## DTC Troubleshooting: 66

DTC 66: | VSA Pressure Sensor (Softwear)

1. | Clear the DTCs using the HDS.

2. | Turn the ignition switch OFF, then turn it ON (II).

3. | Verify the DTC. Is DTC 66 indicated? YES - Go to 4. NO - The system is OK at this time.n

4. | From the HDS Main Menu, select VSA, check VSA BRAKE PRESSER in the FUNCTION TEST. Is the result? YES - Check for loose connector terminals in the VSA control unit 46P connector and repair if necessary. If terminals are OK, replace the VSA modulator-control unit.n NO - Check the brake lines for damage and leaks. Also check for bent brake lines.n