## M/T Mainshaft Bearing and Oil Seal Replacement

Special Tools Required
Adjustable bearing puller, 25-40 mm ( 07JAC-PH80100)

Bearing remover shaft ( 07JAC-PH80200)
Slide hammer ( 07741-0010201)
Driver ( 07749-0010000)
Attachment, 37 x 40 mm ( 07746-0010200)
Attachment, 52 x 55 mm ( 07746-0010400)

1. | Remove the differencial assembly.

2. | Remove the ball bearing (A) from the clutch housing (B) using the special tool.

3. | Remove the oil seal (A) from the clutch side.

4. | Drive the new oil seal in from the transmission side using the special tools.

5. | Drive the new ball bearing (A) in from the transmission side using the special tools.