## Rear Window Defogger Wire Repair

NOTE: To make an effective repair, the broken section must be no longer than one inch.

1. | Lightly rub the area around the broken section (A) with fine steel wool, then clean it with alcohol.

2. | Carefully mask above and below the broken portion of the defogger wire (B) with transparent tape (C).

3. | Using a small brush, apply a heavy coat of silver conductive paint extending about 1/8²on both sides of the break. Allow 30 minutes to dry. Thoroughly mix the paint before use.

4. | Check for continuity in the repaired wire.

5. | Apply a second coat of paint in the same way. Let it dry 3 hours before removing the tape.