## Recirculation Control Motor Replacement

NOTE: LHD type is shown, RHD type is symmetrical.

1. | Turn the ignition switch OFF.

2. | Remove the inner glove box.

3. | Disconnect the 7P connector (A) from the recirculation control motor (B). Remove the self-tapping screws and the recirculation control motor from the blower unit.

4. | Install the motor in the reverse order of removal. Make sure the pin on the motor is properly engaged with the linkage. After installation, make sure the motor runs smoothly.