## Valves, Springs, and Valve Seals Removal

Special Tools Required
Valve spring compressor ( 07757-0010000)

Identify the valves and valve springs as they are removed so that each item can be reinstalled in its original position.

1. | Remove the cylinder head.

2. | Remove the camshaft.

3. | Using an appropriate-sized socket (A) and plastic mallet (B), lightly tap the valve retainer to loosen the valve keepers.

4. | Install the spring compressor. Compress the spring, and remove the valve keepers.