## Air Mix Control Motor Replacement

1. | Remove the passenger's dashboard under cover .

2. | Disconnect the 7P connector (A) from the air mix control motor (B). Remove the self-tapping screws and the air mix control motor from the heater unit.

3. | Install the motor in the reverse order of removal.Make sure the pin on the motor is properly engaged with the linkage. After installation, make sure the motor runs smoothly.