## Driver's Airbag Replacement

## Removal

1. | Disconnect the battery negative cable, and wait at least 3 minutes before beginning work.

2. | Remove the access panel (A) from the steering wheel, then disconnect the connector between the cable reel 4P connector (B) and driver's airbag 4P connector (C).

3. | Remove the two Torx bolts (A) using a Torx T30 bit. Then remove the driver's airbag (B).

## Installation

1. | Place the new driver's airbag (A) in the steering wheel, and secure it with new Torx bolts (B).

2. | Connect the cable reel 4P connector (A) to the driver's airbag 4P connector (B), then install the access panel (C) on the steering wheel.

3. | Connect the battery negative cable.

4. | After installing the airbag, confirm proper system operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off. Make sure the horn button works.