## Front Seat Cushion Removal/Installation

1. | Remove the front seat.

2. | Remove the recline cover and center cover, with manual height, without manual height.

3. | With side airbag: From under the seat cushion, detach the side airbag connector clip. Release the hook springs and harness band.

4. | Release the hooks (A) from both sides the seat cushion.

5. | Release the seat-back cover (A) from the cushion frame spring (B), and release the hooks (C) from under the seat cushion.

6. | Remove the seat cushion cover/pad from the seat cushion frame.

7. | Install the cushion in the reverse order of removal. To prevent wrinkles when installing a seat cushion cover, make sure the material is stretched evenly over the pad before securing the hooks.