## CVT Speed Sensor Replacement

1. | Remove the air cleaner housing and intake air duct.

2. | Disconnect the CVT speed sensor connector.

3. | Remove the CVT speed sensor.

4. | Install the new CVT speed sensor (C) with the new O-ring (B) and the sensor washer (A). When installing the sensor, do not allow dust or other foreign particles to enter the transmission.

5. | Check the connector for rust, dirt, or oil, then connect the connector securely.

6. | Install the air cleaner housing and intake air duct.