## Design Specifications

Item | Measurement | Qualification | Specification
--- | --- | --- | ---
DIMENSION | Overall length |  | 3,830 mm (150.8 in.)
Overall width |  | 1,675 mm (65.9 in.)
Overall height |  | 1,525 mm (60.0 in.)
Wheelbase |  | 2,450 mm (96.5 in.)
Track equipped with 175/65R14 82T tyres | Front | 1,460 mm (57.5 in.)
Rear | 1,445 mm (56.9 in.)
Track equipped with 185/55R15 82V tyres | Front | 1,440 mm (56.7 in.)
Rear | 1,430 mm (56.3 in.)
Ground clearance |  | 140 mm (5.5 in.)
Seating capacity |  | Five (5)
WEIGHT | Curb weight | M/T | 977-1,045 kg (2,154-2,304 lbs)
CVT | 1,018-1,065 kg (2,244-2,348 lbs)
ENGINE | Type | Except L15A1, L15A5, and L15A6 engines | Water-cooled, 4-stroke SOHC i-DSI engine
L15A1, L15A5, and L15A6 engines | Water-cooled, 4-stroke SOHC VTEC engine
Cylinder arrangement |  | Inline 4-cylinder, transverse
Bore and stroke | L12A1, L12A3, and L12A4 engines | 73 x 74.4 mm (2.87 x 2.93 in.)
L13A1, L13A2, L13A3, L13A4, L13A5, and L13A6 engines | 73 x 80 mm (2.87 x 3.15 in.)
L15A1, L15A2, L15A4, L15A5, and L15A6 engines | 73 x 89.4 mm (2.87 x 3.52 in.)
Displacement | L12A1, L12A3, and L12A4engines | 1,246 cm3 (76 cu in.)
L13A1, L13A2, L13A3, L13A4, L13A5, and L13A6 engines | 1,339 cm3 (82 cu in.)
L15A1, L15A2, L15A4, L15A5, and L15A6 engines | 1,496 cm3 (91 cu in.)
Compression ratio | KY (except Esypt), KZ, and KN models | 10.4
KY (Esypt) model | 10.5
Except KY, KZ, and KN models | 10.8
Valve train | L15A1, L15A5, and L15A6 engines | Chain drive, SOHC VTEC 4 valves per cylinder
Except L15A1, L15A5, and L15A6 engines | Chain drive, SOHC 2 valves per cylinder
Lubrication system |  | Forced, wet sump, with trochoid pump
Oil pump displacement | At 6,300 rpm (min-1) | 44.6 L (47.1 US qt, 39.2 Imp qt)
Water pump displacement | At 6,000 rpm (min-1) | 120 L (127 US qt, 106 Imp qt)
Fuel required | KE, KG, KB models | Premium UNLEADED petrol with 95 research octane number or higher
KH, KK, KT, KZ, KN, KU, KQ, KY, KM, KP, FO models | UNLEADED petrol with 91 research octane number or higher
IN model | UNLEADED petrol with 88 research octane number or higher

Item | Measurement | Qualification | Specification
--- | --- | --- | ---
STARTER | Type |  | Gear reduction
Normal output | L12A1, L12A3, L13A1, L13A3, L13A4, and L13A5 engines for M/T model | 0.6 kW
L13A1, L13A3, L13A4, and L13A5 engines for CVT model | 0.7 kW
L12A4 and L13A6 engines | 0.6 kW
L15A1, L15A2, L15A4, L15A5, and L15A6 engines | 0.7 kW
L13A2 engine | 1.0 kW
Hour rating |  | 30 seconds
Rotation direction |  | Clockwise as viewed from gear end
CLUTCH | Clutch type | M/T | Single plate dry, diaphragm spring
CVT | Multi plates wet sump, hydraulic
Clutch friction material surface area | M/T | 143 cm2 (22.1 sq in.)
MANUAL TRANSMISSION | Type |  | Synchronized, 5-speed forward, 1 reverse
Primary reduction |  | Direct 1:1
Gear ratio | 1st | 3.142
2nd | 1.750
3rd | 1.241
4th | 0.969
5th | 0.805
Reverse | 3.230
Final | 4.111
Final reduction | Type | Single helical gear
CVT | Type |  | Electronically controlled continuously variable transmission
Primary reduction |  | Direct 1:1
Gear ratio | Low-High | 2.367-0.407
Reverse | 2.367-1.326
Final reduction | Type | Single helical gear
Gear ratio (Except L15A1, L15A5 engines) | 4.714
Gear ratio (L15A1, L15A5 engines) | 4.333
STEERING | Type |  | Rack and pinion with electrical power-assisted
Overall ratio | Manufactured except HATC | 175/65R14 82T: 17.52
185/55R15 82V: 17.79
Manufactured HATC | 17.79
Turns, lock-to-lock | Manufactured except HATC | 175/65R14 82T: 3.71
185/55R15 82V: 3.53
Manufactured HATC | 3.53
Steering wheel diameter |  | 380 mm (15.0 in.)
SUSPENSION | Type | Front | Independent strut with stabilizer, coil spring
Rear | De Dion axle
Shock absorber | Front | Telescopic, hydraulic, nitrogen gas-filled
Rear | Telescopic, hydraulic, nitrogen gas-filled

(cont'd)
Item | Measurement | Qualification | Specification
--- | --- | --- | ---
BRAKES | Type of service brake | Front | Power-assisted self-adjusting ventilated disc
Rear | Power-assisted self-adjusting solid drum
Type of parking brake |  | Mechanical actuating, rear wheels
Pad friction surface area | Front | 44.5 cm2 (6.90 sq in.) x 2
Shoe friction surface area | Rear | 21.0 cm2 (3.26 sq in.) x 2
TYRES | Size of front and rear tyres |  | 175/65R14 82T
185/55R15 82V
Size of spare tyre |  | T115/70D14 88M
AIR CONDITIONING | Compressor | Type | Scroll
Capacity | 85.7 mL (5.23 cu in.)/rev.
Maximum speed | 12,000 rpm (min-1)
Lubricant capacity | 85 mL (2 1/2 fl oz)
Lubricant type | KEIHIN SP-10
Condenser | Type | Corrugated fin
Evaporator | Type | Corrugated fin
Blower | Type | Radial
Motor type | 220 W/12 V
Speed control | 4-speed
Maximum capacity | 380 m3/h (13,400 cu ft/h)
Temperature control |  | Air-mix type
Compressor clutch | Type | Dry, single plate, Poly V-belt drive
Electrical power consumption at 20 °C ( 68 °F) | 42 W maximum at 12 V
Refrigerant | Type | HFC-134a (R-134a)
Capacity | 400-450 g (14.1-15.9 oz)
ELECTRICAL RATINGS | Battery |  | 12 V-28 AH/5 hours
Starter |  | 12 V-0.6 kW, 0.7 kW, 1.0 kW
Alternator |  | 12 V-75 A
Fuses | Under-hood fuse/relay box | 80 A, 50 A, 40 A, 30 A, 20 A, 15 A, 10 A
Under-dash fuse/relay box | 20 A, 15 A, 10 A, 7.5 A
Light bulbs | Headlight high beam | 12 V-60 W
Headlight low beam | 12 V-55 W (without HID headlight)
12 V-35 W (with HID headlight)
Front turn signal/Front side marker lights | 12 V-21 W
Side turn signal lights | LED (in the power mirror)
Front parking lights | 12 V-5 W
Rear turn signal lights | 12 V-21 W
Brake/Taillights | 12 V-21/5 W
Back-up lights | 12 V-21 W
License plate light | 12 V-5 W
Ceiling light | 12 V-8 W
Tailgate light | 12 V-5 W
Spotlights | 12 V-5 W
Gauge lights | LED
Indicator lights | LED