## Rear Door Latch Replacement

NOTE: Put on gloves to protect your hands.

1. | Raise the glass fully.

2. | Remove these items: Door panel Plastic cover, as necessary Rod protector

3. | Disconnect the lock rod (A) from the lock crank (B).

4. | With Super Locking: Remove the bolts, then remove the harness protector (A).

5. | Disconnect (and detach) the actuator connector (A). Remove the screws securing the latch (B). Take care not to bend the inner handle rod (C) and lock rod (D).

6. | Disconnect the inner handle rod (A) and lock rod (B) from the latch (C).

7. | Remove the bolts (A, B) securing the rear lower channel (C), then remove the collar (D).

8. | Move the latch (A) through the gap between the rear lower channel (B) and door, then remove it.

9. | Install the latch in the reverse order of removal, and note these items: Make sure the connector is plugged in properly, and each rod is connected securely. Make sure the door locks and opens properly.