## Power Window Passenger's Motor Test

1. | Remove the door panel.

2. | Disconnect the 2P connector (A) from the passenger's power window motor.

3. | Test the motor in each direction by connecting battery power and ground according to the table. To prevent damage to the motor, disconnect one lead as soon as the motor stops running.

4. | If the motor does not run or fails to run smoothly, replace it.