## A/C Receiver/Dryer Desiccant Replacement

1. | Remove the condensor.

2. | Remove the mount (A) and the cap (B) from the bottom of the condenser, then remove the O-rings (C), the filter (D) and the desiccant (E).

3. | Install the desiccant in the reverse order of removal, and note these items: Replace the O-rings with new ones, and apply a thin coat of refrigarent oil (KEIHIN SP-10) before installing them. Be sure to use the right O-rings for HFC-134a (R-134a) to avoid leakage.