## Radio Remote Switch Test

1. | Remove the driver's airbag assembly.

2. | Remove the 7P connector (A) from the radio remote switch (B).

3. | Remove the three mounting screws and the switch.

4. | Measure resistance between the No. 5 and No. 6 terminals and between the No. 5 and No. 7 terminals in each switch position according to the table.
Position | Resistance
--- | ---
OFF | About 10 kW
MODE | About 4 kW
CH (+) | About 2 kW
CH (-) | About 840 W
5(VOL. UP) | About 370 W
6(VOL. DOWN) | About 100 W

5. | If the resistance is not as specified, replace the remote switch.