## CVT Flywheel Housing Input Shaft Oil Seal Replacement

Special Tools Required
Handle driver ( 07749-0010000)

Driver attachment, 37 x 40 mm ( 07746-0010200)

1. | Remove the main valve body from the flywheel housing.

2. | Remove the old oil seal from the flywheel housing.

3. | Install the new oil seal flush with the flywheel housing. It is allowed to install the oil seal plus or minus 0.5 mm (0.02 in.) from level.