## Fuse to Component Index

Under-hood fuse/relay box
Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | 80A | ——— | Battery, Power distribution
2 | 40A | WHT/BLU | EPS control unit
3 | 50A | WHT | Ignition switch (BAT)
4 | 40A | WHT/RED | ABS modulator-control unit
5 | 40A | WHT/BLU | Blower motor
6 | 40A | WHT | No. 2, 3, 4, 13 and 14 fuses (in the under-dash fuse/relay box)
7 | 30A | BLU/RED | No.18, 19 and 21 fuses (in the under-dash fuse/relay box), Power mirror defogger, Sunroof motor
8 | 15A | WHT/RED | Audio unit, Ceiling light, Data link connector, Gauge assembly, Immobilizer control unit-receiver, Immobilizer code unit, Keyless receiver unit, Navigation unit, Spotlights, Tailgate light
9 | 10A | RED/BLK | Dash lights, Front parking lights, Gauge lights, License plate lights, Taillights
10 | 30A*6 | BLU/BLK | Radiator fan motor
20A*5
11 | 30A | BLU/YEL | A/C compressor clutch relay
BLU/RED | Condenser fan motor
12 | 20A*1 | RED | Right headlight
15A*2 | RED/WHT | Right headlight (HID unit, switching solenoid)
13 | 20A*1 | RED/YEL | Left headlight, High beam indicator
15A*2 | BLU/RED | Left headlight (HID unit, switching solenoid), High beam indicator
14 | 10A | WHT/BLK | Turn signal/hazard flasher control circuit (Has built in gauge assembly)
15 | 30A | WHT/GRN | ABS modulator-control unit
16 | 15A*3 · 10A*4 | WHT/GRN | ABS modulator-control unit, Brake lights, ECM/PCM, Shift lock control circuit (Has built in gauge assembly)
BLU/RED | Horn
Fuse/relay box socket | Horn relay

*1: | Except KU with HID headlight
*2: | KU with HID headlight
*3: | With trailer lighting connector
*4: | Without trailer lighting connector
*5: | Except KM model
*6: | KM model

Under-dash Fuse/Relay Box
Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | 10A | YEL | Back-up light (M/T)
2 | 15A | BLK/RED | Ignition coil (rear)
3 | 7.5A | YEL | Alternator, EPS control unit, ELD unit, EVAP canister purge valve, Gauge assembly, Headlight adjuster, Headlight adjuster switch, IMOES unit, Keyless receiver unit, Primary HO2S, Sunroof control unit (KK, KY, KU, KT and KN models), Shift lock solenoid (CVT), Secondary HO2S, Vehicle speed sensor (M/T)
4 | 10A | YEL/BLK | Turn signal/hazard flasher circuit (built into gauge assembly)
5 | 7.5A | BLK/RED | ECM (with throttle actuator control)
6 | 20A | GRN/BLK | Intermittent wiper control unit (built into wiper/washer switch), Rear washer motor, Windshield wiper motor, Windshield washer motor
7 | ——— | ——— | Not used
8 | ——— | ——— | Not used
9 | 20A | BLK/ORN | Rear window defogger (via rear window defogger switch)
10 | 7.5A | BLK/YEL | A/C compressor clutch relay, A/C switch, Blower motor relay, Condenser fan relay, Climate control unit, Power mirror actuator, Power mirror defogger relay, Radiator fan relay
Fuse/relay box socket | Optional connector
11 | 15A | BLK/YEL | ECM/PCM, Fuel pump, Inertia switch, Immobilizer control unit-receiver, SRS unit (VA)
12 | 10A | GRN | Power window control unit (built into power window master switch), Rear window wiper motor
Fuse/relay box socket | Power window relay
13 | 10A | PNK | SRS unit (VB)
14 | 15A | WHT/BLK | CKP sensor, TDC sensor, ECM/PCM, Injectors, IAC valve, PGM-FI main relay1, PGM-FI main relay2
15 | 20A | YEL/RED | Left rear power window motor (via power window switch)
16 | 20A | YEL/BLU | Right power window motor (via power window switch)
17 | 20A | GRN/BLK | Front passenger's power window motor (via power window switch)
18 | 10A | WHT/GRN | Rear fog light control unit (with front fog light)
19 | 20A | BLU/RED | Sunroof motor
20 | ——— | ——— | Not used
21 | 20A | BLU/BLK | Front fog light
22 | ——— | ——— | Not used
23 | ——— | ——— | Not used
24 | 15A | BLK/WHT | Ignition coil (front)
25 | 7.5A | YEL | ABS modulator-control unit (IG1)
26 | 7.5A | YEL/RED | Audio unit (without navigation), AVN unit (with navigation), Key interlock solenoid (CVT), Navigation unit
Fuse/relay box socket | Optional connector
27 | 15A | YEL/GRN | Accessory power socket, Cigarette lighter
28 | 20A | WHT | Door lock actuator, Tailgate lock actuator
29 | 20A | GRN/WHT | Driver's power window motor (via power window master switch)