## Under-dash Fuse/Relay Box Removal and Installation

SRS components are located in this area. Review the SRS component locations, and precautions and procedures in the SRS section before performing repairs or service.

## Removal

1. | Disconnect the battery negative cable, then disconnect the positive cable, and wait at least three minutes.

2. | Remove the fuse lid cover.

3. | Disconnect the connectors from the fuse side of the under-dash fuse/relay box.

4. | Remove the mounting nuts (A) and down the under-dash fuse/relay box (B).

5. | Disconnect the connectors from the back of the under-dash fuse/relay box, and remove the fuse/relay box. NOTE: The SRS connector is a spring-loaded lock type.

## Installation

1. | Install the under-dash fuse/relay box in the reverse order of removal and connect all connectors to the under-dash fuse/relay box.

2. | Install the fuse lid cover.

3. | Connect both the negative cable and positive cable to the battery.

4. | Enter the anti-theft code for the radio, then enter the customer's radio station presets.

5. | Confirm that all systems work properly.