## Headlight Replacement

1. | Remove the front bumper.

2. | Disconnect the connectors (A) from the headlight (B).
Headlight: 60/55 W Front Position Light: 5 W Front Turn Signal Light: 21 W

3. | Remove the three mounting bolts and the screw from the headlight.

4. | Remove the bolt and the corner upper beam (C).

5. | Install in the reverse order of removal.

6. | After replacement, adjust the headlights to local requirements.