## Camshaft Installation

1. | Install the camshaft (A) into the cylinder head, then install the camshaft thrust cover (B) with new O-ring (C).

2. | Install the Top Dead Center (TDC) sensor with new O-ring, then connect the TDC sensor connector.

3. | Install the harness holder, then install harness holder mounting bolt, ground cable and air cleaner housing bracket.

4. | Install the camshaft sprocket.

5. | Install the rocker arm assembly.

6. | Install the air cleaner housing.