## A/T Shift Lever Removal

1. | Remove the center console, and remove the heater duct.

2. | Shift into the [N] position.

3. | Remove the nut securing the shift cable end, then separate the cable end from the shift lever.

4. | Rotate the socket holder (A) on the shift cable (B) a quarter turn; the tab (C) on the socket holder will be in the opening of the shift lever bracket base (D). Then slide the holder to remove the shift cable from the shift lever bracket base. Do not remove the shift cable by twisting the shift cable guide (E).

5. | Disconnect the shift lock solenoid connector (A), then remove the harness clamps (B) from the shift lever bracket base.

6. | Remove the shift lever assembly.