## ATF Cooler Hoses Replacement

1. | Insert the ATF hoses (A) over the ATF cooler lines (B) on the transmission until the hoses contact the bracket of the ATF lines.

2. | Install the clips (C) to secure the hoses at 6-8 mm (0.2-0.3 in.) (D) from the hose end.

3. | Install the ATF cooler hoses (E) over the lines (F) on the ATF cooler (G); insert the hoses to the bulge (H) of the lines.

4. | Install the clips (I) to secure the hoses at 2-4 mm (0.1-0.2 in.) (J) from the hose end.