## Rocker Arms and Shaft Inspection

1. | Remove the rocker arm assembly.

2. | Measure the diameter of the shaft at the first rocker location.

3. | Zero the gauge (A) to the shaft diameter.

4. | Measure the inside diameter of the rocker arm, and check it for an out-of-round condition.
Rocker Arm-to-Shaft Clearance:
Standard (New): | 0.019-0.058 mm (0.0007-0.0023 in.)
Service Limit: | 0.08 mm (0.003 in.)

5. | Repeat for all rocker arms and both shafts. If the clearance is over the limit, replace the rocker shaft and all overtolerance rocker arms.