## Starter Replacement

1. | Disconnect the battery negative cable, then disconnect the positive cable.

2. | Remove the splash shield.

3. | Disconnect the starter cable (A) from the B terminal on the solenoid, then disconnect the BLK/WHT wire (B) from the S terminal.

4. | Remove the two bolts holding the starter, then remove the starter.

5. | Install the starter in the reverse order of removal. Make sure the crimped side of the ring terminal (A) is facing out.

6. | Connect the battery positive cable and negative cable to the battery.