## Rear Door Outer Handle Replacement

NOTE : Put on gloves to protect your hands.

1. | Raise the glass fully.

2. | Remove these items: Door panel Plastic cover, as necessary

3. | Release the inner handle rod (A) and lock rod (B) from the rod holder (C).

4. | Remove the screw, and release the hooks (D), then remove the rod protector (E).

5. | Remove the screws securing the latch (A), then move the latch down. Take care not to bend any of the rods.

6. | Remove the bolts securing the outer handle (A) and outer handle protector (B).

7. | Detach the outer handle protector (A) from the handle clip (B) by pulling it back, then remove it from the outer handle (C).

8. | From inside the door, pry the clip (A) catching the edge of the handle opening flange. Pull out the outer handle (B), then remove it.

9. | Install the handle in the reverse order of removal, and note these items: Make sure the door locks and opens properly. Make sure the handle clip catches the edge of the opening flange securely.